

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | |  | | | | |
|  | | | | |
| **QUOTATION** | | | | | | |
|  | |  | |  | |  |
|  | |  | |  | |  |
| Quotation date (valid time: 15days) | | | | 2018.12.10 | | |
| **Project : Modern Prefab House**  (HS code:9406000090 ;picture just for reference ) | | | | | | |
|  | | | | | | |
|  | | | | | | |
| **House Cost** | | | | | | |
| Item | Dimension | Area(㎡) |  | Single Building Price ($) | Quantity (set) | Total price($) |



|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| House | 16.5\*7\*4.9m | 110 |  | $60,369.00 | 1 | $65,000.00 |
| Total Cost | | | | | | $65,000.00 |
| Theporice is CIF ASWP. | | | | | | |
| **Remark** | | **Delivery Time:** 10 days after received 50% deposit, need final confirmation | | | | |
| **Payment:** T/T 50% as deposit, 50% balance before loading from factory | | | | |
| **Loading:** it need final confirmation. | | | | |
| **Installation** | | 1. We can give you the processing drawing to guide the installation. 2. We can send our skill worker to your country to guide work,you need to provide return air tickets; visa cost,accommodation ,salary USD120/day.need to final confirmation 3. You can send your worker to our factory to learn installation. | | | | |
| **Main Material Lists** | | | | | | |
| No. | Component | Materials  **(need to final confirmation ,according to design)** | | | Thickness (mm) | Photo |
| 1 | Pillar | 150 \* 150mm Square Tube | | | 4mm |  |
| 2 | Ring Beam | 100\*100mm Square Tube | | | 3mm |  |
| 3 | Roof Purlin | 40\*80mm Square Tube | | | 2mm |  |
| 4 | Roof Beam | 80\*80mm Square Tube | | | 3mm |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 5 | Wall Panel | PU Sandwich Panel | 100\*950mm |  |
| 6 | Partition Wall Panel | PU Sandwich Panel | 100\*950mm |  |
| 7 | Roof Panel | PU Sandwich Panel | 50\*950mm |  |
| 8 | Roof Tile | Steel Sheet | 0.476mm |  |
| 9 | Ceiling Decoration | Charcoal fiber decoration panel | 200 \*10mm |  |
| 10 | Exterior Wall Decoration | PU Decoration Wall Panel | 3080 \*380mm |  |
| 11 | Interior Wall Decoration | Charcoal fiber decoration panel | 300\*3000mm |  |
| 12 | Floor Decoration | Ceramic TIile | 800\*800mm |  |
| 13 | Door | Glass Aluminum Sliding Door | 4500\*3000mm |  |
| 14 | Window | Glass Aluminum Sliding Window | 1500\*1000mm |  |



|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 15 | Toilet Door | Ecological Door | | 700\*2000mm |  |
| 16 | Accessories | screw,rivet,bolt and sealant etc | | |  |
| 17 | Water & Eletricity | Wires, tubes, sockets, switches | | |  |
| **Exported Countries** | | | | | |
| **Asia** : Korea，India ,malaysia ,Thailad,Kuwait, Jordan ,Indonesia,Qatar,Oman,Philippines | | | **Europe:** Spain,England | | |
| **Africa:** Cameroon, mozambique, Mauritius,Ethiopia Angola,South Africa,Djibouti,Congo | | | **South America:** Trinidad andTobago,Chile, Brazil,Colombia,Bolivia,Suriname,Uruguay, venezuela | | |
| Oceania:Australia ，Kiribati | | |  | | |
| **Technical Parameter** | | | | | |
| No | Project Name | Value | No | Project Name | Value |
| 1 | Roof load | ≧65kilograms/m2 | 5 | Wall deformation | ≦65kilograms/m2 |
| 2 | Flooring load | ≧150kilograms/m2 | 6 | Seismic grade | 7-magnitude |
| 3 | Aisle load | ≧200kilograms/m2 | 7 | Wind loading | ≧100km/h |
| 4 | Wall side stress | ≧80kilograms/m2 | 8 | Fire proof | B1 grade |