|  |  |
| --- | --- |
| **Vehicle Specification** | |
| Make & Model | Toyota Land Cruiser 200 VXR, LHD, 4X4, 363, 5.7L, P, A, B7, 3/4 |
| Trim Level | VXR |
| Steering Configuration | LHD |
| Engine Type | 5.7L V8, 32 VALVE, DOHC, DUAL VVT-I PETROL |
| Transmission | 8-Speed Automatic |
| Drive Type | Fulltime 4X4 with Low Range |
| Seating Capacity | 5 Seats |
| Seating Configuration | 2 + 3 - Leather |
| Seat Belts | 3-Point Seat Belts |
| Engine Power | 363 hp |
| Torque | 529.56 N.m |
| Interior Finishing | OEM |
| Interior Floor Finishing | OEM |
| Fuel Capacity | 138 liters |
| Overall Length | 5,095 mm |
| Overall Width | 1,980 mm |
| Overall Height | 1,900 mm |
| Wheelbase | 2,850 mm |
| Ground Clearance | 230 mm |
| Kerb Weight | 4920 kg |
| Tyres | OEM |
| Suspension | Heavy-Duty Suspension \*BILSTEIN\* |
| Suspension Type | Front & Rear: Coil Spring & Damper \*BILSTEIN\* |
| Axle Configuration (Front) | Independent Double Wishbone |
| Axle Configuration (Rear) | Rigid, Multi-Link With Differential Lock |
| Air Conditioning | OEM, Dual-zone |
| Braking System | Electronic Controlled, Hydraulic ABS |
| Brake Configuration | Front & Rear: Disc |
| Bumper Configuration | OEM |
| Exterior Lighting | Halogen Bulb |
| Interior Lighting | LED with Halogen Bulb |
| System Voltage | 12 Volt |
| Alternator (Kw) | 180Amp |
| Battery Type (V/Ah) | 12V/95Ah CCA 800A |
| **Armoring Specification** | |
| Engine Bay | CEN 1522 FB7: Flanks, Battery, ECU |
| Crew Compartment | CEN 1522 FB7: Doors, Side Walls, Firewall, Bulkead & Roof, 3/4 armoring |
| Floor | 2XDM 51 or equivalent grenades |
| Fuel Tank Protection | 2XDM 51 or equivalent grenades |
| Glass | CEN 1063 BR7: Windshield, Door Glass, Bulkhead Glass |
| Glass Configuration | Windscreen 1 Piece Curved; Doors 1 Piece Curved x 4; Bulkhead 1 Piece Flat |
| Gun-Ports | Rotary |
| Gun-Ports Configuration | 1 gun port in front passenger glass, 1 in each second row passenger glass |
| Door Frame | Large door frame overlaps with anti-spall/ricochet barriers |
| Door Hinges | Heavy Duty |
| Security Locking System | OEM |
| Wheels | Run-Flat x 4 + 1 Spare |
| Hatch | Roof hatch with struts and locking system |
| **Additional Options** | |
| Red and Blue LED Strobe light bar mounted on interior of rear window | |
| Siren and PA System | |
| Fire suppression system in engine compartment manually activated from driver position | |
| Wheel and Tire Upgrade | |
| Suspension Upgraded | |
| Brake Upgrade | |