The common features are:
 
	Transmission
	8 speeds, Automatic

	Brakes
	Brakes: Front: 330x24mm Vented disk - 48mm Twin-piston floating c, Rear: 328x12mm Solid disk - 45mm Single-piston floating

	Drive Type:
	Part-time 4x4 Hi-Lo

	Tyres
	On/off-road A/S Front: P245/75R17 Rear: P245/75R17. 17 x 7.5 in. Michelin / Bridgestone

	Suspensions
	Front: 5-link coil spring, Rear: 5-link coil spring

	Wheelbase
	Standard 3008 mm, Ground Clearance: 246 mm

	Weight
	GVW 2631kg, Kerb Weight 2111kg and payload 520kg

	Seats
	5-Seater. Front: 1+1 3-Way adjustable, Rear: 40/60 3 with headrests and 3-point seatbelts. Material: cloth

	Dimensions
	Length: 4785mm, Width: 1875mm, Height: 1868mm, Volume: 16.8m³ all excluding accessories

	Country of Origin
	United States

	Engine Model
	EXJ-DFV 3.0A - 2987cc, Diesel (Tank 69l), 6 cylinders, BHP: 260, KW: 194, Cooling (Liquid), 12 Volts

	No of doors
	5


 
180 AMP ALTERNATOR
650 AMP AGM BATTERY
STABILITY CONTROL-WITH
HILL START ASSIST
TRACTION CONTROL
ELECTRONIC ROLL MITIGATION
TRAILER SWAY DAMPING
HYDRAULIC ASSIST BRAKE BOOSTER
ANTI-LOCK 4-WHEEL DISC HD BRAKES
LOW BACK BUCKET SEATS
RECLINING FRONT SEATS
DRIVER HEIGHT ADJUSTER SEAT
REAR 60/40 FOLDING SEAT
CHILD SEAT UPPER TETHER ANCHORAGE
RR HEAD RESTRAINTS OUTBOARD SEATING
ADVANCED MULTISTAGE FRONT AIR BAGS
SUPPLEMENTAL FRT SEAT SIDE AIR BAGS
FRONT SEAT AREA CARPET
REAR SEAT/WHEELHOUSE/CARGO CARPET
CARGO TIE DOWN LOOPS
FRONT & REAR FLOOR MATS
SPORT BAR
THREE REAR SEAT HEAD RESTRAINTS
FRONT SEAT BACK MAP POCKETS
DRIVER AND PASSENGER ASSIST HANDLES
FULL LENGTH FLOOR CONSOLE
REAR COMPARTMENT STORAGE TRAY
STORAGE TRAY
URETHANE SHIFT KNOB
ILLUMINATED CUPHOLDERS
COMMAND-TRAC PART TIME 4WD SYSTEM
DANA M220 REAR AXLE
CONVENTIONAL DIFFERENTIAL FRT AXLE
SOLAR CONTROL GLASS
TINTED WINDSHIELD GLASS
FRONT DOOR TINTED GLASS
FULL METAL DOORS W/ROLL-UP WINDOWS
REAR VIEW DAY/NIGHT MIRROR
SLIDING SUN VISORS W/MIRRORS
MANUAL MIRRORS, FOLD-AWAY
SENTRY KEY THEFT DETERRENT SYSTEM
PUSHBUTTON START
AIR CONDITIONING
HOOD INSULATION
CLUSTER 3.5" TFT B&W DISPLAY
120 MPH PRIMARY SPEEDOMETER
SILVER PLATINUM I/P BEZELS
MANUAL DOOR LOCKS
OUTSIDE TEMPERATURE GAUGE
MANUAL WINDOWS
VAR INTERMITTENT WINDSHIELD WIPERS
METHANOL WINDSHIELD WASHER FLUID
DUAL NOTE ELECTROMECHANICAL HORNS
12V AUXILIARY POWER OUTLET
AUXILIARY 12-VOLT REAR POWER OUTLET
LOCKING GLOVE BOX
MANUAL 2-WAY DRIVER LUMBAR ADJUST
MANUAL 6-WAY DRIVER SEAT
FRT PASS SEAT - MANUAL ADJUST 4-WAY
FRONT PASSENGER SEAT BELT ALERT
VEHICLE INFORMATION CENTER
INCANDESCENT TAILLAMPS
COURTESY LAMPS
FRONT DOME W/ON/OFF SWITCH LAMP
BLACK EXTERIOR MIRRORS
HEADLAMP OFF TIME DELAY
REAR DOME W/ON/OFF SWITCH LAMP
HALOGEN HEADLAMPS
FT SIDE MARKER/SIDE REPEATER LAMP
FRONT FOG LAMPS
CHMSL LAMP
MOLDED BLACK FRONT BUMPER
BLOW MOLDED BLACK REAR BUMPER
NON-VENTED HOOD
BLACK FRONT FRAME OVERLAY
BODY COLOR GRILLE
WRANGLER DECAL
MIC FENDER FLARES (1PCS FRT/1PC RR)
BLACK DOOR HANDLES
GRAY/BLACK TRAIL RATED BADGE
JEEP BADGE
SPEED CONTROL
BRIGHT WHITE CLEAR COAT
8 SPEAKERS
FIXED LONG MAST ANTENNA
STEERING WHEEL MOUNTED AUDIO CTRLS
MEDIA HUB (USB, AUX)
AUDIO JACK INPUT FOR MOBILE DEVICES
REMOTE USB PORT
POWER STEERING
STEERING WHEEL
NORMAL DUTY SUSPENSION
FRONT STABILIZER BAR
REAR STABILIZER BAR
BLACK SUNRIDER SOFT TOP
TILT/TELESCOPE STEERING COLUMN
FULL SIZE SPARE TIRE
OUTSIDE TIRE CARRIER
UCONNECT 4 WITH 7" DISPLAY
17X7.5 BLACK STEEL STYLED WHEELS
MATCHING SPARE WHEEL
PARKVIEW REAR BACK-UP CAMERA
OCCUPANT CLASSIFICATION SYSTEM
FUEL TANK SKID PLATE SHIELD
TRANSFER CASE SKID PLATE SHIELD
2 FRONT & 1 REAR TOW HOOKS
TORX TOOL KIT
TRANSMISSION SKID PLATE
R1234YF A/C REFRIGERANT
TIRE PRESSURE MONITORING DISPLAY
TETHERED FUEL FILLER CAP
ENGLISH/USA LANGUAGE
PROTECTIVE COATING AND REMOVER
BASE INTERIOR ACCENTS
BUMPER MODULE I
WHEEL FLARE/DRL PARTS MODULE
GRILLE MODULE
MOPAR CUSTOM SHOP MODULE
DOOR TRIM PANEL MODULE
GLASS MODULE
CENTER CONSOLE PARTS MODULE
FRONT FASCIAS PARTS MODULE
SEAT PARTS MODULE
INSTRUMENT PANEL PARTS MODULE
DOOR PARTS MODULE
FRONT END PARTS MODULE
FRONT SUSPENSION PARTS MODULE
REAR SUSPENSION PARTS MODULE
TIRE & WHEEL PARTS MODULE
FRAME PARTS MODULE
BUILD TO U.S. MKT. SPECIFICATIONS
EMEA REGION ECE
ZONE 06-EXPORT
JL/5403 VEHICLE FAMILY
FOUR WHEEL DRIVE (4WD)/(4X4)
LEFT HAND DRIVE (LHD)
2022 VEHICLE SPECIFICATIONS
FOUR DOOR
VEHICLE ORDER TRACKING
LONG WHEEL BASE (LWB)
U.S. SPECIFICATIONS LABEL
CLOTH LOW-BACK BUCKET SEATS
BLACK
AUX BATTERY
SELEC-SPEED (TM) CONTROL
ALL AUTOMATIC TRANSMISSIONS                   
8-SPD AUTO 8HP75 TRANS (BUY-GERMANY)
DANA M210 FRONT AXLE
3.73 REAR AXLE RATIO
ANTI-SPIN DIFFERENTIAL REAR AXLE
3.0L V6 TURBO DIESEL ENGINE W/ESS G3
110MPH VEHICLE MAX SPEED CALIBRATION
GPS ANTENNA INPUT
GRAY ECODIESEL BADGE
50 STATE EMISSIONS
18.3 GALLON FUEL TANK
BRIGHT WHITE CLEAR COAT
ALL RADIO EQUIPPED VEHICLES
GLOBAL TELEMATICS BOX MODULE (TBM)
7.0" TOUCH SCREEN DISPLAY
APPLE CARPLAY
GOOGLE ANDROID AUTO
USB HOST FLIP
INTEGRATED CENTER STACK RADIO
4G LTE WI-FI HOT SPOT
SIRIUSXM GUARDIAN-INCLUDED TRIAL (B)
ALL VP2 RADIOS
MICHELIN or BRIDGESTONE BRAND TIRES
ALL STEEL WHEELS
SELECTIVE CATALYTIC REDUCTION (UREA)
TIP START
STOP-START DUAL BATTERY SYSTEM
BLACK FUEL FILLER DOOR
NON-LOCK FUEL CAP W/ DISCRIMINATOR
INTEGRATED VOICE COMMAND W/BLUETOOTH
3.8 ADDITIONAL GALLONS OF DIESEL
SPRING - LEFT REAR
SPRING - LEFT FRONT
SPRING - RIGHT REAR
SPRING - RIGHT FRONT
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